* Data management to create database
* Select all vicon cameras
  + Window
    - Camera mode
  + If camera doesn’t come up
    - Right click and reboot
* Mask cameras (takes empty points and ignore them)
  + Click mask
  + Whenever they get blue, stop mask
* Aim camera start
* Calibrate
  + Get wand and place it in the origin
  + Calibration, full calibration
  + Selected cameras
  + 2000
  + 750
  + Auto stop check
  + Press start and move wand to calibrate
  + It will auto stop
  + <0.3 is good in image, <0.1 is better
  + Set wand in origin again
* Set volume origin
  + Press start and set origin
* System tab
  + Core processor
    - Reconstruct
* Subject tab
  + Click 2nd icon
    - Click on ben subject model
* Tools tab and go to the little person and select ben.
  + Start subject capture
  + Pipeline
    - Reconstruct
      * Label
        + Esc
    - File I/O
      * Export ascii delimited
* Save and go live